Now installing across the region

# Your roof is the best investment you already own.

सूर्य आत्मा जगतस्तस्थुषश्च

sūrya ātmā jagatas tasthuṣaś ca·the sun is the soul of all that moves and all that moves not

CloudHelio designs, installs and monitors custom rooftop solar systems engineered to maximize energy efficiency and help lower your electricity costs for decades.

Scroll
Run the numbers

## Move two sliders. See twenty-five years.

Every figure below recalculates live against your bill, your roof and your shading — the same model our surveyors use on site.

Monthly electricity bill₹3,000
Usable roof area 850 sq ft
How much shade does your roof get?
Estimated 25-year net savings
₹7,55,958

After the ₹1,38,000 net install cost is paid back — 3.6 years in, on a system built for a 25-year design lifespan.

₹3,170
Monthly
3.6 yr
Payback
100%
Bill offset
Projected monthly generation
5,138 kWh / year
3.60 kW
J
F
M
A
M
J
J
A
S
O
N
D
Array footprint
8 panels
Roof used 17%

Laid out at 3.60 kW across 850 sq ft, leaving statutory access setbacks clear.

CO₂ avoided over 25 years
91.2 t

Versus grid-average generation for your region.

Equivalent mature trees
174

Absorbing the same carbon every year the array runs.

Install cost after subsidy
₹1,38,000

₹2,16,000 before the ₹78,000 PM Surya Ghar subsidy — we file the paperwork.

Estimates only. Final figures come from your roof survey, tariff and local incentive schedule.

Visual Transformation

## See the SolarMind Difference

Drag the interactive slider below to compare a standard utility-dependent roof against an optimized N-type TOPCon solar array.

BEFORE: Bare Roof & High Utility Bills
AFTER: CloudHelio Rooftop Solar Installed
◀▶
Monthly Utility Cost
₹8,500 → ₹850

90% Instant Bill Cut

Grid Reliance
100% → 10%

Net-metering surplus exports

Property Valuation
Standard → +4.1% Boost

Appraised solar asset value

How it works

## Five weeks from first call to first kilowatt.

The same sequence on every job, with a named project manager who stays with you from survey through commissioning.

01 Day 1

### Remote roof study

We pull satellite imagery and a decade of local irradiance data, then model shading hour by hour across the year. No one visits yet.

02 Day 3–5

### On-roof survey

A structural engineer checks rafter spacing, membrane condition and load path, and confirms the array layout against the model.

03 Week 2

### Permits & interconnection

We file the building permit, utility interconnection agreement and every incentive claim. You sign twice; we handle the rest.

04 Week 5

### Installation

One to two days on site. Flashed mounts, sealed penetrations, conduit run inside where we can. Your power stays on throughout.

05 Ongoing

### Commission & monitor

Panel-level monitoring goes live the day we energise. If a single module underperforms for a week, we see it before you do.

NABCEP-certified installers Fully insured, ₹5 crore liability No subcontracted crews Roof penetrations warranted 25 years
Clear Answers

## Frequently Asked Questions

Everything you need to know about rooftop solar installation, subsidies, and maintenance.

Under PM Surya Ghar Muft Bijli Yojana, residential rooftop systems receive ₹30,000 per kW up to 2 kW (₹60,000) plus ₹18,000 for the 3rd kW, capping at ₹78,000 total. CloudHelio handles all portal filings and DISCOM approvals directly for you.
Free · No obligation

## Find out what your roof is worth.

Three questions, ninety seconds. You'll get a modelled yield estimate, an install cost after incentives, and a payback figure — by email, with no one phoning you unless you ask.

512
  Systems installed
4.9
  Average rating
48h
  Estimate turnaround

1. Property 2. Usage 3. Contact
Property type
Roof construction